**Supplementary Data**

**Table S1**: Recent studies reporting contamination of potentially toxic elements (PTEs) in different water sources (i) rivers/lakes/canals, (ii) groundwater/drinking water, (iii) city wastewater, and (iv) industrial water.

|  |  |  |  |
| --- | --- | --- | --- |
| **Metal** | **Country** | **Concentration (mg/L)** | **Reference** |
| **Rivers/lakes/canals** | | | |
| Al | Dongting Lake, China | 1890 | (Long et al., 2021) |
| Fe | Dongting Lake, China | 26120 | (Long et al., 2021) |
| Zn | Dongting Lake, China | 53320 | (Long et al., 2021) |
| Cu | Dongting Lake, China | 9.1 | (Long et al., 2021) |
| Mo | Dongting Lake, China | 2.9 | (Long et al., 2021) |
| Ni | Dongting Lake, China | 1.7 | (Long et al., 2021) |
| Mn | Dongting Lake, China | 4986 | (Long et al., 2021) |
| Ba | Dongting Lake, China | 98.2 | (Long et al., 2021) |
| Pb | Dongting Lake, China | 21.4 | (Long et al., 2021) |
| Cr | Dongting Lake, China | 43.2 | (Long et al., 2021) |
| As | Dongting Lake, China | 42.6 | (Long et al., 2021) |
| Al | China | 9908 | (Tong et al., 2021) |
| As | China | 48.05 | (Tong et al., 2021) |
| Ba | China | 310 | (Tong et al., 2021) |
| Cd | China | 61.74 | (Tong et al., 2021) |
| Co | China | 42.49 | (Tong et al., 2021) |
| Cr | China | 624 | (Tong et al., 2021) |
| Cu | China | 1100 | (Tong et al., 2021) |
| Fe | China | 68479 | (Tong et al., 2021) |
| Mn | China | 2745 | (Tong et al., 2021) |
| Ni | China | 600 | (Tong et al., 2021) |
| Pb | China | 690 | (Tong et al., 2021) |
| Zn | China | 10600 | (Tong et al., 2021) |
| Cr | China | 5.81 | (Xu et al., 2021) |
| As | China | 1 | (Xu et al., 2021) |
| Cd | China | 0.1 | (Xu et al., 2021) |
| Pb | China | 5 | (Xu et al., 2021) |
| Zn | China | 50 | (Xu et al., 2021) |
| Cu | China | 10 | (Xu et al., 2021) |
| Ni | China | 2 | (Xu et al., 2021) |
| Hg | China | 0.1 | (Xu et al., 2021) |
| Cd | Pakistan | 3 | (Ahmad et al., 2021b) |
| Cr | Afghanistan | 0.02779 | (Zahidi et al., 2020) |
| Mn | Afghanistan | 0.017 | (Zahidi et al., 2020) |
| Fe | Afghanistan | 0.638 | (Zahidi et al., 2020) |
| Ni | Afghanistan | 0.00375 | (Zahidi et al., 2020) |
| Cu | Afghanistan | 0.03235 | (Zahidi et al., 2020) |
| Zn | Afghanistan | 0.05095 | (Zahidi et al., 2020) |
| Cd | Afghanistan | 0.00133 | (Zahidi et al., 2020) |
| Hg | Afghanistan | 0.000723 | (Zahidi et al., 2020) |
| Pb | Afghanistan | 0.00957 | (Zahidi et al., 2020) |
| As | Afghanistan | 0.002509 | (Zahidi et al., 2020) |
| As | Pakistan | 33 | (Ahmad et al., 2021b) |
| As | Pakistan | 33 | (Abbas et al., 2021) |
| Pb | Bangladesh | 0.05 | (Rahman et al., 2020) |
| Cd | Bangladesh | 0.005 | (Rahman et al., 2020) |
| Cd | Bangladesh | 0.05 | (Rahman et al., 2020) |
| Cr | India | 0.66 | (Rizwan et al., 2021) |
| Pb | India | 0.51 | (Rizwan et al., 2021) |
| Co | India | 1.21 | (Rizwan et al., 2021) |
| Fe | India | 0.39 | (Rizwan et al., 2021) |
| Mn | India | 0.97 | (Rizwan et al., 2021) |
| **Groundwater / drinking water** | | | |
| As | Rayong Province, Thailand | 183 | (Nilkarnjanakul et al., 2022) |
| Mg | Rayong Province, Thailand | 49 | (Varol et al., 2021) |
| Na | Rayong Province, Thailand | 39 | (Varol et al., 2021) |
| K | Rayong Province, Thailand | 69 | (Varol et al., 2021) |
| Fe | Rayong Province, Thailand | 5 | (Varol et al., 2021) |
| As | Rayong Province, Thailand | 36 | (Varol et al., 2021) |
| B | Rayong Province, Thailand | 1.55 | (Varol et al., 2021) |
| Al | China | 800 | (Tong et al., 2021) |
| As | China | 262.43 | (Tong et al., 2021) |
| Ba | China | 733 | (Tong et al., 2021) |
| Cd | China | 15 | (Tong et al., 2021) |
| Co | China | 60 | (Tong et al., 2021) |
| Cr | China | 50 | (Tong et al., 2021) |
| Cu | China | 223 | (Tong et al., 2021) |
| Fe | China | 3071 | (Tong et al., 2021) |
| Mn | China | 1300 | (Tong et al., 2021) |
| Ni | China | 62 | (Tong et al., 2021) |
| Pb | China | 136.50 | (Tong et al., 2021) |
| Zn | China | 7400 | (Tong et al., 2021) |
| Cd | Arba Minch, Ethiopia | 0.005 | (Guadie et al., 2021) |
| Cu | Arba Minch, Ethiopia | 0.02 | (Guadie et al., 2021) |
| Fe | Arba Minch, Ethiopia | 2.13 | (Guadie et al., 2021) |
| Mn | Arba Minch, Ethiopia | 0.12 | (Guadie et al., 2021) |
| Pb | Arba Minch, Ethiopia | 0.4 | (Guadie et al., 2021) |
| Zn | Arba Minch, Ethiopia | 0.12 | (Guadie et al., 2021) |
| Cd | China | 0.05825 | (Jiang et al., 2021a) |
| Cr | China | 982.6 | (Jiang et al., 2021a) |
| As | China | 163.8 | (Jiang et al., 2021a) |
| Mn | China | 524.27 | (Jiang et al., 2021a) |
| Fe | China | 1050.84 | (Jiang et al., 2021a) |
| Cu | China | 68.27 | (Jiang et al., 2021a) |
| Zn | China | 257.3 | (Jiang et al., 2021a) |
| Pb | China | 72.84 | (Jiang et al., 2021a) |
| Al | Qorveh, Iran | 8 | (Maleki and Jari, 2021) |
| As | Qorveh, Iran | 54 | (Maleki and Jari, 2021) |
| Cd | Qorveh, Iran | 0.2 | (Maleki and Jari, 2021) |
| Co | Qorveh, Iran | 2 | (Maleki and Jari, 2021) |
| Cr | Qorveh, Iran | 10 | (Maleki and Jari, 2021) |
| Cu | Qorveh, Iran | 28 | (Maleki and Jari, 2021) |
| Fe | Qorveh, Iran | 316 | (Maleki and Jari, 2021) |
| Hg | Qorveh, Iran | 1 | (Maleki and Jari, 2021) |
| Mn | Qorveh, Iran | 12 | (Maleki and Jari, 2021) |
| Mo | Qorveh, Iran | 0.3 | (Maleki and Jari, 2021) |
| Ni | Qorveh, Iran | 0.4 | (Maleki and Jari, 2021) |
| Pb | Qorveh, Iran | 2 | (Maleki and Jari, 2021) |
| Sb | Qorveh, Iran | 0.5 | (Maleki and Jari, 2021) |
| Se | Qorveh, Iran | 29 | (Maleki and Jari, 2021) |
| Zn | Qorveh, Iran | 107 | (Maleki and Jari, 2021) |
| Sn | Qorveh, Iran | 18 | (Maleki and Jari, 2021) |
| Al | Qorveh, Iran | 8 | (Maleki and Jari, 2021) |
| As | Qorveh, Iran | 47 | (Maleki and Jari, 2021) |
| Cd | Qorveh, Iran | 0.2 | (Maleki and Jari, 2021) |
| Co | Qorveh, Iran | 0.2 | (Maleki and Jari, 2021) |
| Cr | Qorveh, Iran | 53 | (Maleki and Jari, 2021) |
| Cu | Qorveh, Iran | 27 | (Maleki and Jari, 2021) |
| Fe | Qorveh, Iran | 240 | (Maleki and Jari, 2021) |
| Hg | Qorveh, Iran | 0.4 | (Maleki and Jari, 2021) |
| Mn | Qorveh, Iran | 6.7 | (Maleki and Jari, 2021) |
| Mo | Qorveh, Iran | 0.3 | (Maleki and Jari, 2021) |
| Ni | Qorveh, Iran | 5.3 | (Maleki and Jari, 2021) |
| Pb | Qorveh, Iran | 0.4 | (Maleki and Jari, 2021) |
| Sb | Qorveh, Iran | 0.6 | (Maleki and Jari, 2021) |
| Se | Qorveh, Iran | 20 | (Maleki and Jari, 2021) |
| Zn | Qorveh, Iran | 65 | (Maleki and Jari, 2021) |
| Sn | Qorveh, Iran | 2 | (Maleki and Jari, 2021) |
| Al | Bijar, Iran | 30 | (Maleki and Jari, 2021) |
| As | Bijar, Iran | 26 | (Maleki and Jari, 2021) |
| Cd | Bijar, Iran | 0.2 | (Maleki and Jari, 2021) |
| Co | Bijar, Iran | 1 | (Maleki and Jari, 2021) |
| Cr | Bijar, Iran | 11 | (Maleki and Jari, 2021) |
| Cu | Bijar, Iran | 27 | (Maleki and Jari, 2021) |
| Fe | Bijar, Iran | 54 | (Maleki and Jari, 2021) |
| Hg | Bijar, Iran | 1 | (Maleki and Jari, 2021) |
| Mn | Bijar, Iran | 0.2 | (Maleki and Jari, 2021) |
| Mo | Bijar, Iran | 0.3 | (Maleki and Jari, 2021) |
| Ni | Bijar, Iran | 0.4 | (Maleki and Jari, 2021) |
| Pb | Bijar, Iran | 4 | (Maleki and Jari, 2021) |
| Sb | Bijar, Iran | 0.6 | (Maleki and Jari, 2021) |
| Se | Bijar, Iran | 24 | (Maleki and Jari, 2021) |
| Zn | Bijar, Iran | 88 | (Maleki and Jari, 2021) |
| Sn | Bijar, Iran | 14 | (Maleki and Jari, 2021) |
| Al | Bijar, Iran | 27 | (Maleki and Jari, 2021) |
| As | Bijar, Iran | 27 | (Maleki and Jari, 2021) |
| Cd | Bijar, Iran | 0.2 | (Maleki and Jari, 2021) |
| Co | Bijar, Iran | 0.7 | (Maleki and Jari, 2021) |
| Cr | Bijar, Iran | 9.2 | (Maleki and Jari, 2021) |
| Cu | Bijar, Iran | 27 | (Maleki and Jari, 2021) |
| Fe | Bijar, Iran | 27 | (Maleki and Jari, 2021) |
| Hg | Bijar, Iran | 1 | (Maleki and Jari, 2021) |
| Mn | Bijar, Iran | 0.2 | (Maleki and Jari, 2021) |
| Mo | Bijar, Iran | 0.3 | (Maleki and Jari, 2021) |
| Ni | Bijar, Iran | 0.2 | (Maleki and Jari, 2021) |
| Pb | Bijar, Iran | 7 | (Maleki and Jari, 2021) |
| Sb | Bijar, Iran | 0.6 | (Maleki and Jari, 2021) |
| Se | Bijar, Iran | 19 | (Maleki and Jari, 2021) |
| Zn | Bijar, Iran | 66 | (Maleki and Jari, 2021) |
| Sn | Bijar, Iran | 12 | (Maleki and Jari, 2021) |
| As | Divandare, Iran | 1 | (Maleki and Jari, 2021) |
| Cd | Divandare, Iran | 0.2 | (Maleki and Jari, 2021) |
| Cr | Divandare, Iran | 5 | (Maleki and Jari, 2021) |
| Cu | Divandare, Iran | 0.23 | (Maleki and Jari, 2021) |
| Fe | Divandare, Iran | 49 | (Maleki and Jari, 2021) |
| Pb | Divandare, Iran | 5 | (Maleki and Jari, 2021) |
| Se | Divandare, Iran | 13 | (Maleki and Jari, 2021) |
| Zn | Divandare, Iran | 55 | (Maleki and Jari, 2021) |
| As | Divandare, Iran | 1 | (Maleki and Jari, 2021) |
| Cd | Divandare, Iran | 0.2 | (Maleki and Jari, 2021) |
| Cr | Divandare, Iran | 10 | (Maleki and Jari, 2021) |
| Cu | Divandare, Iran | 9.5 | (Maleki and Jari, 2021) |
| Fe | Divandare, Iran | 67 | (Maleki and Jari, 2021) |
| Pb | Divandare, Iran | 14.3 | (Maleki and Jari, 2021) |
| Se | Divandare, Iran | 12 | (Maleki and Jari, 2021) |
| Zn | Divandare, Iran | 28 | (Maleki and Jari, 2021) |
| Zn | Kenya | 0.73 | (Ochiba, 2020) |
| Pb | Kenya | 0.42 | (Ochiba, 2020) |
| Hg | Kenya | 0.0019 | (Ochiba, 2020) |
| Mn | Kenya | 0.26 | (Ochiba, 2020) |
| Cd | Kenya | 0.001 | (Ochiba, 2020) |
| Cr | Kenya | 0.005 | (Ochiba, 2020) |
| Cr | Pakistan | 0.38 | (Rashid et al., 2021) |
| Ni | Pakistan | 0.26 | (Rashid et al., 2021) |
| Cd | Pakistan | 0.08 | (Rashid et al., 2021) |
| Mn | Pakistan | 0.27 | (Rashid et al., 2021) |
| Cu | Pakistan | 0.36 | (Rashid et al., 2021) |
| Pb | Pakistan | 0.22 | (Rashid et al., 2021) |
| Co | Pakistan | 0.04 | (Rashid et al., 2021) |
| Fe | Pakistan | 0.86 | (Rashid et al., 2021) |
| Zn | Pakistan | 0.43 | (Rashid et al., 2021) |
| As | Pakistan | 10 | (Murtaza et al., 2020b) |
| As | Pakistan | 11 | (Murtaza et al., 2020b) |
| As | Pakistan | 50 | (Murtaza et al., 2020b) |
| As | Pakistan | 46.9 | (Sarwar et al., 2020) |
| As | Pakistan | 121.7 | (Bibi et al., 2021) |
| Pb | Pakistan | 0.14 | (Khalid et al., 2020) |
| Cd | Pakistan | 0.01 | (Khalid et al., 2020) |
| Ni | Pakistan | 0.09 | (Khalid et al., 2020) |
| Cu | Pakistan | 0.31 | (Khalid et al., 2020) |
| Mn | Pakistan | 0.94 | (Khalid et al., 2020) |
| Fe | Pakistan | 1.67 | (Khalid et al., 2020) |
| Zn | Pakistan | 2.63 | (Khalid et al., 2020) |
| Cd | India | 0.07 | (Idrees et al., 2018) |
| Cd | Egypt | 0.01 | (Abdalla and Khalil, 2018) |
| As | Pakistan | 46.8 | (Murtaza et al., 2020a) |
| As | Pakistan | 75 | (Murtaza et al., 2020a) |
| As | Pakistan | 51.4 | (Murtaza et al., 2020a) |
| Cd | Pakistan | 100 | (Abbas et al., 2021) |
| Pb | Pakistan | 100 | (Abbas et al., 2021) |
| As | Pakistan | 33 | (Abbas et al., 2021) |
| Pb | Malaysia | 0.005 | (Zainol et al., 2021) |
| Fe | Malaysia | 6.035 | (Zainol et al., 2021) |
| Cu | Malaysia | 0.002 | (Zainol et al., 2021) |
| Ni | Malaysia | 0.003 | (Zainol et al., 2021) |
| Cd | Malaysia | 0.001 | (Zainol et al., 2021) |
| Cr | Malaysia | 0.001 | (Zainol et al., 2021) |
| Zn | Malaysia | 0.023 | (Zainol et al., 2021) |
| Zn | Nigeria | 3.93 | (Ganiyu et al., 2021) |
| Pb | Nigeria | 0.65 | (Ganiyu et al., 2021) |
| Cd | Nigeria | 0.50 | (Ganiyu et al., 2021) |
| Fe | Nigeria | 1.69 | (Ganiyu et al., 2021) |
| Ni | Italy | 0.08 | (Nigro et al., 2017) |
| Ni | Finland | 1.48 | (Heikkinen et al., 2002) |
| Mn | Nigeria | 0.03 | (Ganiyu et al., 2021) |
| Fe | Bangladesh | 5.702 | (Islam and Mostafa, 2021) |
| Cr | Bangladesh | 0.031 | (Islam and Mostafa, 2021) |
| Mn | Bangladesh | 1.614 | (Islam and Mostafa, 2021) |
| Co | Bangladesh | 0.0325 | (Islam and Mostafa, 2021) |
| Cd | Bangladesh | 0.0019 | (Islam and Mostafa, 2021) |
| Pb | Bangladesh | 0.043 | (Islam and Mostafa, 2021) |
| Cu | Bangladesh | 1.07 | (Islam and Mostafa, 2021) |
| B | Bangladesh | 0.866 | (Islam and Mostafa, 2021) |
| Zn | Bangladesh | 1.50 | (Islam and Mostafa, 2021) |
| Cd | Yemen | 0.001 | (Alansi et al., 2021) |
| Fe | Yemen | 0.28 | (Alansi et al., 2021) |
| Ni | Yemen | 0.002 | (Alansi et al., 2021) |
| Pb | Yemen | 0.1 | (Alansi et al., 2021) |
| Zn | Yemen | 0.048 | (Alansi et al., 2021) |
| Co | Yemen | 0.002 | (Alansi et al., 2021) |
| Mn | Yemen | 0.05 | (Alansi et al., 2021) |
| Cu | Yemen | 0.03 | (Alansi et al., 2021) |
| Cr | China | 0.05825 | (Zhang and Wang, 2021) |
| Cu | China | 0.26878 | (Zhang and Wang, 2021) |
| Zn | China | 0.0298 | (Zhang and Wang, 2021) |
| Ni | China | 0.2661 | (Zhang and Wang, 2021) |
| Cd | China | 0.252 | (Zhang and Wang, 2021) |
| Cr | China | 0.02154 | (Lou et al., 2017) |
| Zn | China | 0.05407 | (Lou et al., 2017) |
| Pb | Bangladesh | 0.023 | (Hossain et al., 2020) |
| Co | Bangladesh | 0.2482 | (Hossain et al., 2020) |
| Zn | Bangladesh | 0.015 | (Hossain et al., 2020) |
| Fe | Bangladesh | 0.345 | (Hossain et al., 2020) |
| Cu | Bangladesh | 0.0375 | (Hossain et al., 2020) |
| Mn | Bangladesh | 0.406 | (Hossain et al., 2020) |
| Cu | Pakistan | 2 | (Yaqub et al., 2021) |
| Cr | Pakistan | 1.35 | (Yaqub et al., 2021) |
| Co | Pakistan | 1.86 | (Yaqub et al., 2021) |
| Ni | Pakistan | 0.024 | (Jalees et al., 2021) |
| Zn | Pakistan | 0.028 | (Jalees et al., 2021) |
| Cd | Pakistan | 0.003 | (Jalees et al., 2021) |
| Cr | Pakistan | 3.981 | (Jalees et al., 2021) |
| Pb | Pakistan | 1.804 | (Jalees et al., 2021) |
| Pb | Nigeria | 0.05 | (Olagunju et al., 2020) |
| Cd | Nigeria | 0.04 | (Olagunju et al., 2020) |
| Cr | Nigeria | 0.02 | (Olagunju et al., 2020) |
| Ni | Nigeria | 0.03 | (Olagunju et al., 2020) |
| Cu | Nigeria | 0.05 | (Olagunju et al., 2020) |
| Fe | Nigeria | 0.06 | (Olagunju et al., 2020) |
| Zn | Nigeria | 0.08 | (Olagunju et al., 2020) |
| Cd | Indonesia | 0.002 | (Sholehhudin et al., 2021) |
| Zn | Indonesia | 0.020 | (Sholehhudin et al., 2021) |
| Mn | Indonesia | 1.80 | (Sholehhudin et al., 2021) |
| Cd | Nigeria | 0.012 | (Imam et al., 2021) |
| Co | Nigeria | 0.05 | (Imam et al., 2021) |
| Ni | Nigeria | 0.02 | (Imam et al., 2021) |
| As | China | 0.3 | (Luo et al., 2021) |
| As | Pakistan | 0.015 | (Maskooni et al., 2020) |
| Cd | Pakistan | 0.3036 | (Maskooni et al., 2020) |
| Zn | Pakistan | 4.06 | (Maskooni et al., 2020) |
| Cr | Pakistan | 0.4027 | (Maskooni et al., 2020) |
| Mn | Pakistan | 0.138 | (Maskooni et al., 2020) |
| As | Pakistan | 0.035 | (Aliaskari and Schäfer, 2021) |
| Mn | Nigeria | 63.45 | (Obasi and Akudinobi, 2020) |
| Pb | Nigeria | 11.42 | (Obasi and Akudinobi, 2020) |
| Cr | Nigeria | 14.60 | (Obasi and Akudinobi, 2020) |
| Ni | Nigeria | 1.26 | (Obasi and Akudinobi, 2020) |
| Cd | Nigeria | 15.67 | (Obasi and Akudinobi, 2020) |
| Ag | Nigeria | 6.06 | (Obasi and Akudinobi, 2020) |
| Hg | Nigeria | 2.60 | (Obasi and Akudinobi, 2020) |
| As | Nigeria | 4.13 | (Obasi and Akudinobi, 2020) |
| Co | Nigeria | 0.9 | (Obasi and Akudinobi, 2020) |
| Zn | Nigeria | 10.53 | (Obasi and Akudinobi, 2020) |
| As | India | 1.36 | (Poonia et al., 2021) |
| Cr | India | 33.80 | (Poonia et al., 2021) |
| Cd | Germany | 0.98 | (Kubier et al., 2020) |
| Cr | Morocco | 0.065 | (Lotfi et al., 2020) |
| Fe | Morocco | 0.45 | (Lotfi et al., 2020) |
| Cu | Morocco | 2.9 | (Lotfi et al., 2020) |
| Zn | Morocco | 3.39 | (Lotfi et al., 2020) |
| Cd | Arba Minch, Ethiopia | 0.6 | (Guadie et al., 2021) |
| Cu | Arba Minch, Ethiopia | 0.27 | (Guadie et al., 2021) |
| Fe | Arba Minch, Ethiopia | 6.6 | (Guadie et al., 2021) |
| Mn | Arba Minch, Ethiopia | 0.45 | (Guadie et al., 2021) |
| Pb | Arba Minch, Ethiopia | 1.8 | (Guadie et al., 2021) |
| Zn | Arba Minch, Ethiopia | 0.3 | (Guadie et al., 2021) |
| Pb | Vehari, Pakistan | 0.29 | (Sarwar et al., 2020) |
| Cd | Vehari, Pakistan | 0.03 | (Sarwar et al., 2020) |
| Ni | Vehari, Pakistan | 0.08 | (Sarwar et al., 2020) |
| Cu | Vehari, Pakistan | 1.18 | (Sarwar et al., 2020) |
| Mn | Vehari, Pakistan | 0.43 | (Sarwar et al., 2020) |
| Zn | Vehari, Pakistan | 1.24 | (Sarwar et al., 2020) |
| Fe | Vehari, Pakistan | 4.62 | (Sarwar et al., 2020) |
| **Industrial wastewater** | | | |
| Pb | Tetrapak, Kenya | 29.5 | (Kinuthia et al., 2020) |
| Pb | Chief’s Camp, Kenya | 28.2 | (Kinuthia et al., 2020) |
| Pb | Davis & Shirtliff, Kenya | 24.2 | (Kinuthia et al., 2020) |
| Cr | Sinai, Kenya | 50.7 | (Kinuthia et al., 2020) |
| Cr | Chief’s Camp, Kenya | 9.8 | (Kinuthia et al., 2020) |
| Cd | Railways Lower, Kenya | 0.17 | (Kinuthia et al., 2020) |
| Cd | Davis & Shirtliff, Kenya | 0.13 | (Kinuthia et al., 2020) |
| Cd | Chief’s Camp, Kenya | 0.11 | (Kinuthia et al., 2020) |
| Ni | Railways Lower, Kenya | 21.1 | (Kinuthia et al., 2020) |
| Cu | Taian, China | 90 | (Kinuthia et al., 2020) |
| Zn | Taian, China | 75 | (Kinuthia et al., 2020) |
| Fe | Taian, China | 600 | (Kinuthia et al., 2020) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.34 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.78 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.24 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.82 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.92 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.32 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.94 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.39 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.7 | (Jiku et al., 2021) |
| Cd | Gazipur and Savar industrial Zones, Bangladesh | 0.63 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.63 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 2.01 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.78 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.63 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.22 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.02 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 2.04 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 2.12 | (Jiku et al., 2021) |
| Pb | Gazipur and Savar industrial Zones, Bangladesh | 1.17 | (Jiku et al., 2021) |
| Fe | Gazipur and Savar industrial Zones, Bangladesh | 1.46 | (Jiku et al., 2021) |
| Fe | Gazipur and Savar industrial Zones, Bangladesh | 1.07 | (Jiku et al., 2021) |
| Fe | Gazipur and Savar industrial Zones, Bangladesh | 1.20 | (Jiku et al., 2021) |
| Fe | Gazipur and Savar industrial Zones, Bangladesh | 1.14 | (Jiku et al., 2021) |
| Fe | Gazipur and Savar industrial | 1.78 | (Jiku et al., 2021) |
| Mn | Gazipur and Savar industrial | 1.32 | (Jiku et al., 2021) |
| Mn | Gazipur and Savar industrial | 1.2 | (Jiku et al., 2021) |
| Cu | Gazipur and Savar industrial | 1.56 | (Jiku et al., 2021) |
| Cu | Gazipur and Savar industrial | 1.32 | (Jiku et al., 2021) |
| Cu | Gazipur and Savar industrial | 1.14 | (Jiku et al., 2021) |
| Cu | Gazipur and Savar industrial | 3.52 | (Jiku et al., 2021) |
| **City wastewater** | | | |
| Cd | Arba Minch, Ethiopia | 0.6 | (Guadie et al., 2021) |
| Cu | Arba Minch, Ethiopia | 0.27 | (Guadie et al., 2021) |
| Fe | Arba Minch, Ethiopia | 6.6 | (Guadie et al., 2021) |
| Mn | Arba Minch, Ethiopia | 0.45 | (Guadie et al., 2021) |
| Pb | Arba Minch, Ethiopia | 1.8 | (Guadie et al., 2021) |
| Zn | Arba Minch, Ethiopia | 0.3 | (Guadie et al., 2021) |
| Pb | Vehari, Pakistan | 0.29 | (Sarwar et al., 2020) |
| Cd | Vehari, Pakistan | 0.03 | (Sarwar et al., 2020) |
| Ni | Vehari, Pakistan | 0.08 | (Sarwar et al., 2020) |
| Cu | Vehari, Pakistan | 1.18 | (Sarwar et al., 2020) |
| Mn | Vehari, Pakistan | 0.43 | (Sarwar et al., 2020) |
| Zn | Vehari, Pakistan | 1.24 | (Sarwar et al., 2020) |
| Fe | Vehari, Pakistan | 4.62 | (Sarwar et al., 2020) |

**Table S2**: Removal efficiency and/or adsorption capacity of various MOFs for potentially toxic metal(loid)-contaminated wastewaters.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Materials** | **Metal** | **Q** | **mg/g** | **pH** | **Reference** |
| CS grafted UiO-66-NH2 | Cu | − | 364.96 | − | (Hu et al., 2022) |
| CS grafted UiO-66-NH2 | Pb | − | 555.56 | − | (Hu et al., 2022) |
| Co-MOF | Ce | − | 93.3 | 1.01-5.1 | (Khalil et al., 2022) |
|  | Eu | − | 27.47 | 1.01-5.1 | (Khalil et al., 2022) |
| UiO-66-EDTMPA | Pb | − | 558.67 | − | (Yan et al., 2022) |
|  | Cd | − | 271.34 | − | (Yan et al., 2022) |
|  | Cu | − | 210.89 | − | (Yan et al., 2022) |
| Fe3O4@ZIF-8 | Pb | 98 | 719.42 | 1.0-7.0 | (Jiang et al., 2021b) |
| Fe3O4@ZIF-9 | Cu | 98 | 301.33 | 1.0-7.0 | (Jiang et al., 2021b) |
| Cu-MOF-74 | Cd | 95 | 150 | 6.5 | (Kim et al., 2021) |
| Zr-MOF | Cd | − | 37 | 3.0-9.0 | (Nimbalkar and Bhat, 2021) |
| Zr-MOF | Pb | − | 100 | 3.0-9.0 | (Nimbalkar and Bhat, 2021) |
| ZIF-8 | Pb | − | 700 | − | (Tanihara et al., 2021) |
| MoS4-MOF | Hg | 99.9 | − | − | (Yazdi et al., 2021) |
| MIL-53(Al)-1 | F | − | 75.5 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-2 | F | − | 65 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-3 | F | − | 69.6 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-4 | F | − | 72.5 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-5 | F | − | 50.27 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-6 | F | − | 40.34 | 1.0-12.0 | (Huang et al., 2021) |
| MIL-53(Al)-7 | F | − | 35.63 | 1.0-12.0 | (Huang et al., 2021) |
| Fe-MIL-88NH2 | Pb | 72.5 | 250 | 3.0-7.0 | (Fu et al., 2021) |
| Zr-BTC | Fe | − | 5 | 2.0-12.0 | (Jeyaseelan et al., 2021) |
| Fe-BTC | Fe | − | 4.95 | 2.0-12.0 | (Jeyaseelan et al., 2021) |
| Al-BTC | Fe | − | 4.9 | 2.0-12.0 | (Jeyaseelan et al., 2021) |
| ZIF-8 | Pb | 96 | 1780 | 2.0-12.0 | (Ahmad et al., 2021a) |
| ZIF-67 | Pb | 99.5 | 1975 | 2.0-12.0 | (Ahmad et al., 2021a) |
| ZIF-8 | Hg | 93 | 1290 | 2.0-12.0 | (Ahmad et al., 2021a) |
| ZIF-67 | Hg | 94 | 1450 | 2.0-12.0 | (Ahmad et al., 2021a) |
| UiO-66-EDA | Pb | 99 | 243.9 | 2.0-9.0 | (Ahmadijokani et al., 2021) |
| UiO-66-EDA | Cd | 99 | 208.33 | 1.5-7.0 | (Ahmadijokani et al., 2021) |
| UiO-66-EDA | Cu | 99 | 217.39 | 1.5-7.0 | (Ahmadijokani et al., 2021) |
| Mag MOF-NH2 | U | 90.37 | 80 | 2.0-9.0 | (Chen et al., 2021) |
| Fe-MIL-88B | Sb | 95 | 566.1 | 2.0-9.0 | (Chen et al., 2021) |
| Fe-MIL-88B | Sb | 90 | 318.9 | 2.0-9.0 | (Chen et al., 2021) |
| UiO-66@ABs | Cr | 99 | 2.181 | 2.0-12.0 | (Daradmare et al., 2021) |
| TMU-81 | Cd | 98 | 526 | 4.0 | (Esrafili et al., 2021) |
| TMU-81 | Cu | 98 | 200 | 4.0 | (Esrafili et al., 2021) |
| TMU-81 | Cr | 98 | 270 | 4.0 | (Esrafili et al., 2021) |
| TMU-81 | Zn | 98 | 95 | 4.0 | (Esrafili et al., 2021) |
| TMU-81 | Pb | 98 | 60 | 4.0 | (Esrafili et al., 2021) |
| Cu-BTC | Pb | 85 | 230 | 2.0-6.0 | (Hasankola et al., 2019) |
| Cu-BTC | Hg | 35 | − | 2.0-6.0 | (Hasankola et al., 2019) |
| ZIF-67/BC/CH | Cu | − | 200 | 2.0-6.0 | (Li et al., 2020) |
| ZIF-8/PAN | Cu | 96.14 | 250 | 2.0-6.0 | (Li et al., 2020) |
| ZIF-8@SnO2@CoFe2O4 | Ni | 96.5 | 95 | 2.0-7.0 | (Roudbari et al., 2021) |
| PCN-221 | Hg | 98 | 375 | 2.0-10.0 | (Hasankola et al., 2020) |
| UiO-66 | Pb | 89 | − |  | (Lei et al., 2019) |
| ZIF-67@Fe3O4@ESM | Cu | 99 | 285 | 4.0-6.0 | (Mahmoodi et al., 2019) |
| Zn(Bim)(OAc)-NS | Cu | − | 325 | 1.0-13.0 | (Xu et al., 2020) |
| AMCA-MIL-53(Al) | Pb | 79.5 | 390 | 1.47-8.13 | (Alqadami et al., 2018) |
| melamine-MOFs | Pb | − | 122 | 2.0-6.0 | (Yin et al., 2018) |
| melamine-MOFs | Pb | − | 205 | 2.0-6.0 | (Yin et al., 2018) |
| MOF-808-EDTA | La | 99 | 205 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Pr | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Nd | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Ce | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Eu | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Gd | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Zr | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Fe | 99 | 170 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Mn | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Hg | 99 | 592 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Rh | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Ru | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Cd | 99 | 525 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Pb | 99 | 313 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Sn | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Zn | 99 | 210 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Cu | 99 | 180 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Co | 99 | 190 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Ni | 99 | 190 | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Pt | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Pd | 99 | − | 2.0 | (Peng et al., 2018) |
| MOF-808-EDTA | Sb | 99 | − | 2.0 | (Peng et al., 2018) |
| ZIF-8 | Pb | 99 | 1119.8 | 5.1 | (Huang et al., 2018) |
| ZIF-67 | Pb | 99 | 1348.42 | 5.1 | (Huang et al., 2018) |
| ZIF-8 | Cu | 99 | 454.72 | 5.2 | (Huang et al., 2018) |
| ZIF-67 | Cu | 99 | 617.51 | 5.2 | (Huang et al., 2018) |
| Cu-MOFs/Fe3O4 | Pb | 96 | 219 | − | (Shi et al., 2018) |
| La-MGs | Sb | 92.1 | 897.6 | − | (You et al., 2022) |
| MOF-199@PANI, core@shell | Cu | − | 7831.34 | − | (Yuan et al., 2022a) |
| UiO-66-NH2 | Cu | − | 364.96 | − | (Hu et al., 2022) |
| UiO-66-NH2 | Pb | − | 555.56 | − | (Hu et al., 2022) |
| UiO-66-GMA | Pb | 92 | − | − | (Gul Zaman et al., 2022) |
| UiO-66-GMA | Cd | 94 | − | − | (Gul Zaman et al., 2022) |
| UiO-66-GMA | Cu | 96 | − | − | (Gul Zaman et al., 2022) |
| Fe3O4@C-GO-MOF | Pb | − | 344.83 | − | (Wang et al., 2022) |
| Dawsonite (NH2-MIL-53(Al)) | Cu | − | 228.25 | − | (Li et al., 2020) |
| Zr-MOFs | Cu | − | 59.8 | − | (Wang et al., 2018) |
| ZnO-NP@Zn-MOF-74 | Cu | − | 137.17 | − | (Guo et al., 2021) |
| Zr-MOF | Cu | − | 79.34 | − | (Subramaniyam et al., 2022) |
| ZIF-8 | Cu | − | 454.7 | − | (Huang et al., 2018) |
| ZIF-8@GO | Cu | − | 482.29 | − | (Li and Xu, 2021) |
| ZIF-8@GO | Pb | − | 1119.80 | − | (Li and Xu, 2021) |
| Fe3O4@ZIF-8 | Cu | − | 719.42 | − | (Jiang et al., 2021c) |
| Fe3O4@ZIF-8 | Pb | − | 301.33 | − | (Jiang et al., 2021c) |
| CelloZIFPaper | Cd | − | 143 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Cu | − | 354 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Fe | − | 260.8 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Pb | − | 307.3 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Co | − | 350 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Cd | − | 196.8 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Cu | − | 166.5 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Fe | − | 66.2 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Pb | − | 87.2 | 4 | (Abdelhamid et al., 2022) |
| CelloZIFPaper | Co | − | 300 | 4 | (Abdelhamid et al., 2022) |
| TMU-56 | Pb | − | 1130 | − | (Afshariazar et al., 2020) |
| TMU-23 | Pb | − | 434.7 | − | (Shayegan et al., 2020) |

**Table S3**: Removal capacity of various MOFs (2022 only) for PTE-contaminated wastewaters under varied pH levels.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MOF** | **Metal** | **R%** | **pH** | **Reference** |
| UiO-66-GMA | Pb | 22 | 1 | (Gul Zaman et al., 2022) |
| 35 | 2 |
| 45 | 3 |
| 68 | 4 |
| 80 | 5 |
| 92 | 6 |
| 78 | 7 |
| 75 | 8 |
| 70 | 9 |
| UiO-66-GMA | Cd | 32 | 1 | (Gul Zaman et al., 2022) |
| 43 | 2 |
| 58 | 3 |
| 75 | 4 |
| 92 | 5 |
| 96 | 6 |
| 90 | 7 |
| 82 | 8 |
| 80 | 9 |
| Zn-Ph-D CP | Cu | 68 | 5 | (Elewa et al., 2022) |
| 99 | 7 |
| 99 | 9 |
| Fe3O4@ZIF-8 | Cd | 23 | 4 | (Abdel-Magied et al., 2022) |
| 24 | 4.5 |
| 25.5 | 5 |
| 27 | 5.5 |
| 27.5 | 6 |
| Fe3O4@ZIF-8 | Pb | 33 | 4 | (Abdel-Magied et al., 2022) |
| 35 | 4.5 |
| 37 | 5 |
| 37 | 5.5 |
| 36.5 | 6 |
| Fe3O4@UiO-66–NH2 | Cd | 31 | 4 | (Abdel-Magied et al., 2022) |
| 32.5 | 4.5 |
| 33 | 5 |
| 34 | 5.5 |
| 35 | 6 |
| Fe3O4@UiO-66–NH2 | Pb | 36.5 | 4 | (Abdel-Magied et al., 2022) |
| 37 | 4.5 |
| 39 | 5 |
| 39.5 | 5.5 |
| 39.5 | 6 |
| UiO-66-EDA | Pb | 56 | 2 | (Ahmadijokani et al., 2021) |
| 73 | 3 |
| 90 | 4 |
| 95 | 5 |
| 97 | 6 |
| 99 | 7 |
| UiO-66-EDA | Cd | 59 | 2 | (Ahmadijokani et al., 2021) |
| 65 | 3 |
| 74 | 4 |
| 89 | 5 |
| 93 | 6 |
| 96 | 7 |
| UiO-66-EDA | Cu | 62 | 2 | (Ahmadijokani et al., 2021) |
| 68 | 3 |
| 76 | 4 |
| 79 | 5 |
| 92 | 6 |
| 96 | 7 |
| MFZ | Cd | 20 | 1 | (Li et al., 2022) |
| 25 | 2 |
| 31 | 3 |
| 52 | 4 |
| 75 | 5 |
| 88 | 6 |
| 99.9 | 7 |

**Table S4**: Removal capacity of various MOFs (2022 only) for PTE-contaminated wastewaters under varied exposure tomes (minutes).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **MOF** | **Metal** | **Adsorption mg/g** | **R%** | **Time** | **Reference** |
| UiO-66-GMA | Pb | 860 | 86 | 1 | (Gul Zaman et al., 2022) |
| 862 | 86 | 40 |
| 865 | 86 | 80 |
| 875 | 87 | 120 |
| 880 | 88 | 160 |
| 880 | 88 | 200 |
| UiO-66-GMA | Cd | 900 | 90 | 1 | (Gul Zaman et al., 2022) |
| 905 | 90.5 | 40 |
| 910 | 91 | 80 |
| 915 | 92 | 120 |
| 930 | 93 | 160 |
| 950 | 95 | 200 |
| CelloZIFPaper | Co | 100 |  | 1 | (Abdelhamid et al., 2022) |
| 150 | 5 |
| 160 | 10 |
| 200 | 25 |
| 350 | 50 |
| 350 | 200 |
| 350 | 300 |
| 350 | 700 |
| MOF(Zn-Ph-D-CP) | Cu |  | 59 | 1 | (Elewa et al., 2022) |
| 59 | 4 |
| 60 | 8 |
| 68 | 12 |
| 68 | 16 |
| 68 | 20 |
| 68 | 24 |
| UiO-66-Cl | Fe3+ | 1.5 |  | 20 | (Yuan et al., 2022b) |
| 2.5 | 40 |
| 3.5 | 60 |
| 4.5 | 90 |
| 5 | 120 |
| 5.5 | 150 |
| 6 | 180 |
| 6.2 | 240 |
| 6.4 | 360 |
| 6.5 | 480 |
| UiO-66-S | Fe3+ | 6.5 |  | 20 | (Yuan et al., 2022b) |
| 8.5 | 40 |
| 9.5 | 60 |
| 9.6 | 90 |
| 9.7 | 120 |
| 9.8 | 150 |
| 9.8 | 180 |
| 9.8 | 240 |
| 9.8 | 360 |
| 9.8 | 480 |
| Fe3O4@ZIF-8 | Cd | 7 |  | 5 | (Abdel-Magied et al., 2022) |
| 11 | 15 |
| 13 | 30 |
| 17.5 | 45 |
| 22 | 60 |
| 25 | 120 |
| 26 | 180 |
| 27.5 | 300 |
| 27.5 | 480 |
| 27.5 | 960 |
| 27.5 | 1200 |
| 27.5 | 1440 |
| Fe3O4@ZIF-8 | Pb | 8 |  | 5 | (Abdel-Magied et al., 2022) |
| 16 | 15 |
| 25 | 30 |
| 32 | 45 |
| 34 | 60 |
| 36 | 120 |
| 37 | 180 |
| 38 | 300 |
| 38 | 480 |
| 38 | 960 |
| 38 | 1200 |
| 38 | 1440 |
| Fe3O4@UiO-66–NH2 | Cd | 7 |  | 5 | (Abdel-Magied et al., 2022) |
| 13 | 15 |
| 16 | 30 |
| 20 | 45 |
| 23 | 60 |
| 31 | 120 |
| 33 | 180 |
| 34 | 300 |
| 35 | 480 |
| 35 | 960 |
| 35 | 1200 |
| 35 | 1440 |
| Fe3O4@UiO-66–NH2 | Pb | 7 |  | 5 | (Abdel-Magied et al., 2022) |
| 9 | 15 |
| 14 | 30 |
| 18 | 45 |
| 24 | 60 |
| 31 | 120 |
| 33 | 180 |
| 37 | 300 |
| 38 | 480 |
| 39 | 960 |
| 39 | 1200 |
| 39 | 1440 |
| UiO-66-EDA | Cu | 55 | 42 | 20 | (Ahmadijokani et al., 2021) |
| 60 | 46 | 40 |
| 70 | 55 | 60 |
| 78 | 68 | 80 |
| 85 | 72 | 100 |
| 95 | 78 | 120 |
| 100 | 81 | 140 |
| 101 | 82 | 160 |
| 102 | 83 | 180 |
| 103 | 84 | 200 |
| 104 | 85 | 220 |
| 105 | 86 | 240 |
| 106 | 87 | 260 |
| 107 | 88 | 280 |
| 108 | 88 | 300 |
| 109 | 88 | 320 |
| 110 | 89 | 340 |
| 110 | 89 | 360 |
| UiO-66-EDA | Cd | 52 | 48 | 20 | (Ahmadijokani et al., 2021) |
| 60 | 57 | 40 |
| 68 | 62 | 60 |
| 78 | 70 | 80 |
| 88 | 78 | 100 |
| 95 | 82 | 120 |
| 100 | 83 | 140 |
| 101 | 84 | 160 |
| 102 | 84 | 180 |
| 103 | 84 | 200 |
| 104 | 85 | 220 |
| 105 | 86 | 240 |
| 106 | 87 | 260 |
| 107 | 88 | 280 |
| 108 | 89 | 300 |
| 108 | 90 | 320 |
| 109 | 91 | 340 |
| 110 | 91 | 360 |
| UiO-66-EDA | Pb | 50 | 40 | 20 | (Ahmadijokani et al., 2021) |
| 56 | 45 | 40 |
| 62 | 48 | 60 |
| 75 | 59 | 80 |
| 79 | 62 | 100 |
| 95 | 72 | 120 |
| 100 | 78 | 140 |
| 108 | 85 | 160 |
| 114 | 91 | 180 |
| 115 | 92 | 200 |
| 116 | 93 | 220 |
| 120 | 94 | 240 |
| 121 | 95 | 260 |
| 121 | 95 | 280 |
| 122 | 96 | 300 |
| 122 | 96 | 320 |
| 123 | 97 | 340 |
| 123 | 97 | 360 |

**Table S5**: Removal capacity of various MOFs (2022 only) for PTE-contaminated wastewaters under varied MOF applied levels.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MOF** | **Metal** | **R%** | **MOF dose** | **Reference** |
| UiO-66-GMA | Pb | 78 | 0.5 | (Gul Zaman et al., 2022) |
| 92 | 1.0 |
| 96 | 1.5 |
| 95 | 2.0 |
| 94 | 2.5 |
| 94 | 3.0 |
| UiO-66-GMA | Cd | 74 | 0.5 | (Gul Zaman et al., 2022) |
| 86 | 1.0 |
| 94 | 1.5 |
| 95 | 2.0 |
| 94 | 2.5 |
| 94 | 3.0 |
| Zn-Ph-D CP | Cu | 85 | 0.005 | (Elewa et al., 2022) |
| 88 | 0.01 |
| 93 | 0.015 |
| UiO-66-EDA | Cu | 74 | 0.1 | (Ahmadijokani et al., 2021) |
| 76 | 0.4 |
| 78 | 0.6 |
| 80 | 0.75 |
| 83 | 1.0 |
| 84 | 1.5 |
| 87 | 2 |
| 90 | 3 |
| UiO-66-EDA | Cd | 80 | 0.1 | (Ahmadijokani et al., 2021) |
| 83 | 0.4 |
| 86 | 0.6 |
| 89 | 0.75 |
| 91 | 1.0 |
| 9235 | 1.5 |
| 94 | 2 |
| 97.5 | 3 |
| UiO-66-EDA | Pb | 81 | 0.1 | (Ahmadijokani et al., 2021) |
| 84 | 0.4 |
| 89 | 0.6 |
| 95.5 | 0.75 |
| 97 | 1.0 |
| 98 | 1.5 |
| 99 | 2 |
| 99.9 | 3 |

**Table S6**: Removal capacity of various MOFs (2022 only) for PTE-contaminated wastewaters under varied PTE levels.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **MOF** | **Metal** | **Adsorption mg/g** | **R%** | **PTE dose** | **Reference** |
| UiO-66-GMA | Pb | 10 |  | 10 | (Gul Zaman et al., 2022) |
| 100 | 50 |
| 260 | 100 |
| 310 | 200 |
| 380 | 300 |
| 385 | 500 |
| 390 | 750 |
| 400 | 1000 |
| UiO-66-GMA | Cd | 10 |  | 10 | (Gul Zaman et al., 2022) |
| 90 | 50 |
| 210 | 100 |
| 270 | 200 |
| 300 | 300 |
| 320 | 500 |
| 325 | 750 |
| 325 | 1000 |
| CelloZIFPape | Pb | 205 |  | 5 | (Abdelhamid et al., 2022) |
| 420 | 12 |
| 525 | 25 |
| 610 | 50 |
| 750 | 100 |
| MOF(Zn-Ph-D-CP) | Cu |  | 93 |  | (Elewa et al., 2022) |
| 92 |
| 94 |
| 95 |
| Fe3O4@ZIF-8 | Cd | 20 |  | 1 | (Abdel-Magied et al., 2022) |
| 28 | 2.5 |
| 80 | 8 |
| 120 | 18 |
| 140 | 28 |
| Fe3O4@ZIF-8 | Pb | 37 | 1 | (Abdel-Magied et al., 2022) |
| 70 | 2.5 |
| 160 | 8 |
| 205 | 18 |
| 230 | 28 |
| Fe3O4@UiO-66-NH2 | Cd | 28 | 1 | (Abdel-Magied et al., 2022) |
| 70 | 2.5 |
| 160 | 8 |
| 220 | 18 |
| 280 | 28 |
| Fe3O4@UiO-66-NH2 | Pb | 30 | 1 | (Abdel-Magied et al., 2022) |
| 80 | 2.5 |
| 200 | 8 |
| 270 | 18 |
| 320 | 28 |

**Table S7**: Alterations in surface area (m2/g) and pore volume (cm3/g) after postsynthetic functionalization of MOFs. Minus sign indicates % decrease.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MOF** | **Functionalized-MOF** | **Functionalizing element** | **Before** | | **After** | | **% Change** | | **Reference** |
| **Surface Area (m2/g)** | **Pore volume (cm3/g)** | **Surface Area (m2/g)** | **Pore volume (cm3/g)** | **Surface Area (m2/g)** | **Pore volume (cm3/g)** |
| UiO-66-NH2 | UiO-66-GMA | Glycidyl methacrylate (GMA) | 1127 | 0.48 | 1045 | 0.37 | -8 | -30 | (Molavi et al., 2018) |
| MIL-101(Cr) | MIL-101(Cr)- Cyanex | Bis(2,4,4-trimethylpentyl) phosphinic acid (Cyanex®-272) | 3341 | 1.80 | 442 | 0.19 | -656 | -847 | (Keshavarz et al., 2022) |
| MIL-101(Cr) | MIL-101(Cr)-HDEHP | Bis(2-ethylhexyl) hydrogen phosphate (D2EHPA or HDEHP) | 3341 | 1.80 | 1028 | 0.47 | -225 | -283 | (Keshavarz et al., 2022) |
| MIL-101(Cr) | MIL-101(Cr)-TBP | Tributyl phosphate (TBP) | 3341 | 1.80 | 1158 | 0.57 | -189 | -216 | (Keshavarz et al., 2022) |
| ZIF-8 | MFZ | Fe3O4 loading | 983.44 | 0.443 | 371.09 | 0.319 | -165 | -39 | (Li et al., 2022) |
| Zn-MOF | Zn-MOF-500 | Carbonization | 1.11 | 0.0031 | 18.57 | 0.0677 | 94 | 95 | (Zhang et al., 2022) |

**References**

Abbas, Z., Imran, M., Natasha, N., Murtaza, B., Amjad, M., Shah, N.S., Khan, Z.U.H., Ahmad, I., Ahmad, S., 2021. Distribution and health risk assessment of trace elements in ground/surface water of Kot Addu, Punjab, Pakistan: a multivariate analysis. Environmental Monitoring and Assessment 193, 1-11.

Abdalla, F., Khalil, R., 2018. Potential effects of groundwater and surface water contamination in an urban area, Qus City, Upper Egypt. Journal of African Earth Sciences 141, 164-178.

Abdel-Magied, A.F., Abdelhamid, H.N., Ashour, R.M., Fu, L., Dowaidar, M., Xia, W., Forsberg, K., 2022. Magnetic metal-organic frameworks for efficient removal of cadmium(II), and lead(II) from aqueous solution. Journal of Environmental Chemical Engineering 10, 107467.

Abdelhamid, H.N., Georgouvelas, D., Edlund, U., Mathew, A.P., 2022. CelloZIFPaper: Cellulose-ZIF hybrid paper for heavy metal removal and electrochemical sensing. Chemical Engineering Journal 446, 136614.

Afshariazar, F., Morsali, A., Wang, J., Junk, P.C., 2020. Highest and fastest removal rate of PbII ions through rational functionalized decoration of a metal–organic framework cavity. Chemistry–A European Journal 26, 1355-1362.

Ahmad, K., Ashfaq, M., Shah, S.S.A., Hussain, E., Naseem, H.A., Parveen, S., Ayub, A., 2021a. Effect of metal atom in zeolitic imidazolate frameworks (ZIF-8 & 67) for removal of Pb2+ & Hg2+ from water. Food and chemical toxicology 149, 112008.

Ahmad, S., Imran, M., Murtaza, B., Arshad, M., Nawaz, R., Waheed, A., Hammad, H.M., Naeem, M.A., Shahid, M., Niazi, N.K., 2021b. Hydrogeochemical and health risk investigation of potentially toxic elements in groundwater along River Sutlej floodplain in Punjab, Pakistan. Environmental Geochemistry and Health, 1-15.

Ahmadijokani, F., Tajahmadi, S., Bahi, A., Molavi, H., Rezakazemi, M., Ko, F., Aminabhavi, T.M., Arjmand, M., 2021. Ethylenediamine-functionalized Zr-based MOF for efficient removal of heavy metal ions from water. Chemosphere 264, 128466.

Alansi, R.Q., Mohammed, A.M., Ali, M.M., Mokbel Ghalib, W.A., Ponnappa, S.C., 2021. Determination of Heavy Metals in Groundwater Around Al-Buraihi Sewage Station in Taiz City, Yemen. Journal of Health Pollution 11, 210604.

Aliaskari, M., Schäfer, A.I., 2021. Nitrate, arsenic and fluoride removal by electrodialysis from brackish groundwater. Water Research 190, 116683.

Alqadami, A.A., Khan, M.A., Siddiqui, M.R., Alothman, Z.A., 2018. Development of citric anhydride anchored mesoporous MOF through post synthesis modification to sequester potentially toxic lead (II) from water. Microporous and Mesoporous Materials 261, 198-206.

Bibi, I., Natasha, Shahid, M., Niazi, N.K., Younas, F., Naqvi, S.R., Shaheen, S.M., Imran, M., Wang, H., Hussaini, K.M., Zhang, H., 2021. Hydrogeochemical and health risk evaluation of arsenic in shallow and deep aquifers along the different floodplains of Punjab, Pakistan. Journal of Hazardous Materials 402, 124074.

Chen, W., Cai, Y., Lv, Z., Wang, X., Feng, J., Fang, M., Tan, X., 2021. Improvement of U (VI) removal by tuning magnetic metal organic frameworks with amine ligands. Journal of Molecular Liquids 334, 116495.

Daradmare, S., Xia, M., Kim, J., Park, B.J., 2021. Metal–organic frameworks/alginate composite beads as effective adsorbents for the removal of hexavalent chromium from aqueous solution. Chemosphere 270, 129487.

Elewa, K., Belal, A., El Monayeri, O., Tawfic, A.F., 2022. Application of metal-organic framework (Zn-Ph-D CP) for copper ion removal from aqueous solution. Ain Shams Engineering Journal 13, 101670.

Esrafili, L., Firuzabadi, F.D., Morsali, A., Hu, M.-L., 2021. Reuse of predesigned dual-functional metal organic frameworks (DF-MOFs) after heavy metal removal. Journal of Hazardous Materials 403, 123696.

Fu, Q., Lou, J., Peng, L., Zhang, R., Zhou, S., Wu, P., Yan, W., Mo, C., Luo, J., 2021. Iron based metal organic framework for efficient removal of Pb2+ from wastewater. Journal of Solid State Chemistry 300, 122188.

Ganiyu, S.A., Oyadeyi, A.T., Adeyemi, A.A., 2021. Assessment of heavy metals contamination and associated risks in shallow groundwater sources from three different residential areas within Ibadan metropolis, southwest Nigeria. Applied Water Science 11, 1-20.

Guadie, A., Yesigat, A., Gatew, S., Worku, A., Liu, W., Ajibade, F.O., Wang, A., 2021. Evaluating the health risks of heavy metals from vegetables grown on soil irrigated with untreated and treated wastewater in Arba Minch, Ethiopia. Science of The Total Environment 761, 143302.

Gul Zaman, H., Baloo, L., Rahman Kutty, S., Altaf, M., 2022. Post Synthetic Modification of NH2-(Zr-MOF) via Rapid Microwave-Promoted Synthesis for Effective Adsorption of Pb(II) and Cd(II). Arabian Journal of Chemistry, 104122.

Guo, Z., Yang, F., Yang, R., Sun, L., Li, Y., Xu, J., 2021. Preparation of novel ZnO-NP@Zn-MOF-74 composites for simultaneous removal of copper and tetracycline from aqueous solution. Separation and Purification Technology 274, 118949.

Hasankola, Z.S., Rahimi, R., Safarifard, V., 2019. Rapid and efficient ultrasonic-assisted removal of lead (II) in water using two copper-and zinc-based metal-organic frameworks. Inorganic Chemistry Communications 107, 107474.

Hasankola, Z.S., Rahimi, R., Shayegan, H., Moradi, E., Safarifard, V., 2020. Removal of Hg2+ heavy metal ion using a highly stable mesoporous porphyrinic zirconium metal-organic framework. Inorganica Chimica Acta 501, 119264.

Heikkinen, P., Korkka-Niemi, K., Lahti, M., Salonen, V.-P., 2002. Groundwater and surface water contamination in the area of the Hitura nickel mine, Western Finland. Environmental Geology 42, 313-329.

Hossain, S.M.S., Haque, M.E., Pramanik, M.A.H., Uddin, M.J., Al Harun, M.A.Y., 2020. Assessing the groundwater quality and health risk: A case study on Setabganj sugar mills limited, Dinajpur, Bangladesh. Water Science 34, 110-123.

Hu, S.-z., Huang, T., Zhang, N., Lei, Y.-z., Wang, Y., 2022. Chitosan-assisted MOFs dispersion via covalent bonding interaction toward highly efficient removal of heavy metal ions from wastewater. Carbohydrate Polymers 277, 118809.

Huang, L., Yang, Z., Alhassan, S.I., Luo, Z., Song, B., Jin, L., Zhao, Y., Wang, H., 2021. Highly efficient fluoride removal from water using 2D metal-organic frameworks MIL-53 (Al) with rich Al and O adsorptive centers. Environmental Science and Ecotechnology 8, 100123.

Huang, Y., Zeng, X., Guo, L., Lan, J., Zhang, L., Cao, D., 2018. Heavy metal ion removal of wastewater by zeolite-imidazolate frameworks. Separation and Purification Technology 194, 462-469.

Idrees, N., Tabassum, B., Abd\_Allah, E.F., Hashem, A., Sarah, R., Hashim, M., 2018. Groundwater contamination with cadmium concentrations in some West U.P. Regions, India. Saudi Journal of Biological Sciences.

Imam, M.M., Abubakar, F., Muhammad, Z., 2021. Determination of Some Heavy Metals from Ground Water Samples Obtained from Selected Motor Parks in Kaduna, Nigeria. International Journal of Economy, Energy and Environment 6, 81.

Islam, M.S., Mostafa, M., 2021. Groundwater Quality and Risk Assessment of Heavy Metal Pollution in Middle-West Part of Bangladesh. Journal of Earth and Environmental Science Research. SRC/JEESR-158. DOI: <https://doi>. org/10.47363/JEESR/2021 (3) 143, 3.

Jalees, M.I., Farooq, M.U., Shah, A.T., 2021. Cancer risk assessment and modeling of groundwater contamination near industrial estate, Lahore, Pakistan. Journal of Water, Sanitation and Hygiene for Development 11, 314-326.

Jeyaseelan, A., Albaqami, M.D., Viswanathan, N., 2021. Facile design of metal ion fabricated benzene-1, 3, 5-tricarboxylic acid based metal organic frameworks for defluoridation of water. Journal of Environmental Chemical Engineering 9, 104995.

Jiang, C., Zhao, Q., Zheng, L., Chen, X., Li, C., Ren, M., 2021a. Distribution, source and health risk assessment based on the Monte Carlo method of heavy metals in shallow groundwater in an area affected by mining activities, China. Ecotoxicology and Environmental Safety 224, 112679.

Jiang, X., Su, S., Rao, J., Li, S., Lei, T., Bai, H., Wang, S., Yang, X., 2021b. Magnetic metal-organic framework (Fe3O4@ ZIF-8) core-shell composite for the efficient removal of Pb (II) and Cu (II) from water. Journal of Environmental Chemical Engineering 9, 105959.

Jiang, X., Su, S., Rao, J., Li, S., Lei, T., Bai, H., Wang, S., Yang, X., 2021c. Magnetic metal-organic framework (Fe3O4@ZIF-8) core-shell composite for the efficient removal of Pb(II) and Cu(II) from water. Journal of Environmental Chemical Engineering 9, 105959.

Jiku, M.A.S., Singha, A., Faruquee, M., Rahaman, M.A., Alam, M.A., Ehsanullah, M., 2021. Toxic wastewater status for irrigation usage at Gazipur and Savar industrial vicinity of Bangladesh. Acta Ecologica Sinica 41, 358-364.

Keshavarz, F., Kavun, V., van der Veen, M.A., Repo, E., Barbiellini, B., 2022. Molecular-level understanding of highly selective heavy rare earth element uptake by organophosphorus modified MIL-101(Cr). Chemical Engineering Journal 440, 135905.

Khalid, S., Natasha, Shahid, M., Shah, A.H., Saeed, F., Ali, M., Qaisrani, S.A., Dumat, C., 2020. Heavy metal contamination and exposure risk assessment via drinking groundwater in Vehari, Pakistan. Environmental Science and Pollution Research 27, 39852-39864.

Khalil, M., Shehata, M.M., Ghazy, O., Waly, S.A., Ali, Z.I., 2022. Synthesis, characterization and γ-rays irradiation of cobalt-based metal-organic framework for adsorption of Ce(III) and Eu(III) from aqueous solution. Radiation Physics and Chemistry 190, 109811.

Kim, Y., Kim, K., Eom, H.H., Su, X., Lee, J.W., 2021. Electrochemically-assisted removal of cadmium ions by redox active Cu-based metal-organic framework. Chemical Engineering Journal 421, 129765.

Kinuthia, G.K., Ngure, V., Beti, D., Lugalia, R., Wangila, A., Kamau, L., 2020. Levels of heavy metals in wastewater and soil samples from open drainage channels in Nairobi, Kenya: community health implication. Scientific Reports 10, 8434.

Kubier, A., Hamer, K., Pichler, T., 2020. Cadmium background levels in groundwater in an area dominated by agriculture. Integrated environmental assessment and management 16, 103-113.

Lei, C., Gao, J., Ren, W., Xie, Y., Abdalkarim, S.Y.H., Wang, S., Ni, Q., Yao, J., 2019. Fabrication of metal-organic frameworks@ cellulose aerogels composite materials for removal of heavy metal ions in water. Carbohydrate polymers 205, 35-41.

Li, D., Tian, X., Wang, Z., Guan, Z., Li, X., Qiao, H., Ke, H., Luo, L., Wei, Q., 2020. Multifunctional adsorbent based on metal-organic framework modified bacterial cellulose/chitosan composite aerogel for high efficient removal of heavy metal ion and organic pollutant. Chemical Engineering Journal 383, 123127.

Li, D., Xu, F., 2021. Removal of Cu (II) from aqueous solutions using ZIF-8@GO composites. Journal of Solid State Chemistry 302, 122406.

Li, J., Liao, L., Jia, Y., Tian, T., Gao, S., Zhang, C., Shen, W., Wang, Z., 2022. Magnetic Fe3O4/ZIF-8 optimization by Box-Behnken design and its Cd(II)-adsorption properties and mechanism. Arabian Journal of Chemistry 15, 104119.

Long, X., Liu, F., Zhou, X., Pi, J., Yin, W., Li, F., Huang, S., Ma, F., 2021. Estimation of spatial distribution and health risk by arsenic and heavy metals in shallow groundwater around Dongting Lake plain using GIS mapping. Chemosphere 269, 128698.

Lotfi, S., Chakit, M., Belghyti, D., 2020. Groundwater Quality and Pollution Index for Heavy Metals in Saïs Plain, Morocco. Journal of Health and Pollution 10.

Lou, S., Liu, S., Dai, C., Tao, A., Tan, B., Ma, G., Chalov, R.S., Chalov, S.R., 2017. Heavy metal distribution and groundwater quality assessment for a coastal area on a Chinese Island. Polish Journal of Environmental Studies 26.

Luo, C., Routh, J., Luo, D., Wei, L., Liu, Y., 2021. Arsenic in the Pearl River Delta and its related waterbody, South China: occurrence and sources, a review. Geoscience Letters 8, 1-13.

Mahmoodi, N.M., Taghizadeh, M., Taghizadeh, A., Abdi, J., Hayati, B., Shekarchi, A.A., 2019. Bio-based magnetic metal-organic framework nanocomposite: Ultrasound-assisted synthesis and pollutant (heavy metal and dye) removal from aqueous media. Applied Surface Science 480, 288-299.

Maleki, A., Jari, H., 2021. Evaluation of drinking water quality and non-carcinogenic and carcinogenic risk assessment of heavy metals in rural areas of Kurdistan, Iran. Environmental Technology & Innovation 23, 101668.

Maskooni, E.K., Naseri-Rad, M., Berndtsson, R., Nakagawa, K., 2020. Use of heavy metal content and modified water quality index to assess groundwater quality in a semiarid area. Water 12, 1115.

Molavi, H., Eskandari, A., Shojaei, A., Mousavi, S.A., 2018. Enhancing CO2/N2 adsorption selectivity via post-synthetic modification of NH2-UiO-66(Zr). Microporous and Mesoporous Materials 257, 193-201.

Murtaza, B., Amjad, M., Shahid, M., Imran, M., Shah, N.S., Abbas, G., Naeem, M.A., 2020a. Compositional and health risk assessment of drinking water from health facilities of District Vehari, Pakistan. Environmental geochemistry and health 42, 2425-2437.

Murtaza, B., Nazeer, H., Amjad, M., Imran, M., Shahid, M., Shah, N.S., Farooq, A.B.U., Murtaza, G., 2020b. Hydrogeochemical investigation of arsenic in drinking water of schools and age dependent risk assessment in Vehari District, Punjab Pakistan: a multivariate analysis. Environmental Science and Pollution Research 27, 30530-30541.

Nigro, A., Sappa, G., Barbieri, M., 2017. Application of boron and tritium isotopes for tracing landfill contamination in groundwater. Journal of Geochemical Exploration 172, 101-108.

Nilkarnjanakul, W., Watchalayann, P., Chotpantarat, S., 2022. Spatial distribution and health risk assessment of As and Pb contamination in the groundwater of Rayong Province, Thailand. Environmental Research 204, 111838.

Nimbalkar, M.N., Bhat, B.R., 2021. Simultaneous adsorption of methylene blue and heavy metals from water using Zr-MOF having free carboxylic group. Journal of Environmental Chemical Engineering 9, 106216.

Obasi, P.N., Akudinobi, B.B., 2020. Potential health risk and levels of heavy metals in water resources of lead–zinc mining communities of Abakaliki, southeast Nigeria. Applied Water Science 10, 1-23.

Ochiba, N.K., 2020. Assessment Of Levels Of Selected Heavy Metals In Borehole Water In Ongata Rongai, Kajiado County, Kenya. University Of Nairobi.

Olagunju, T., Olagunju, A., Akawu, I., Ugokwe, C., 2020. Quantification and Risk Assessment of Heavy Metals in Groundwater and Soil of Residential Areas around Awotan Landfill, Ibadan, South-west-Nigeria. J Toxicol Risk Assess 6, 033.

Peng, Y., Huang, H., Zhang, Y., Kang, C., Chen, S., Song, L., Liu, D., Zhong, C., 2018. A versatile MOF-based trap for heavy metal ion capture and dispersion. Nature communications 9, 1-9.

Poonia, T., Singh, N., Garg, M., 2021. Contamination of Arsenic, Chromium and Fluoride in the Indian groundwater: a review, meta-analysis and cancer risk assessment. International Journal of Environmental Science and Technology, 1-12.

Rahman, M.A.T., Paul, M., Bhoumik, N., Hassan, M., Alam, M.K., Aktar, Z., 2020. Heavy metal pollution assessment in the groundwater of the Meghna Ghat industrial area, Bangladesh, by using water pollution indices approach. Applied Water Science 10, 1-15.

Rashid, A., Ayub, M., Javed, A., Khan, S., Gao, X., Li, C., Ullah, Z., Sardar, T., Muhammad, J., Nazneen, S., 2021. Potentially harmful metals, and health risk evaluation in groundwater of Mardan, Pakistan: Application of geostatistical approach and geographic information system. Geoscience Frontiers 12, 101128.

Rizwan, K.M., Thirukumaran, V., Suresh, M., 2021. Assessment and source identification of heavy metal contamination of groundwater using geospatial technology in Gadilam River basin, Tamil Nadu, India. Applied Water Science 11, 1-24.

Roudbari, R., Keramati, N., Ghorbani, M., 2021. Porous nanocomposite based on metal-organic framework: Antibacterial activity and efficient removal of Ni (II) heavy metal ion. Journal of Molecular Liquids 322, 114524.

Sarwar, T., Shahid, M., Natasha, Khalid, S., Shah, A.H., Ahmad, N., Naeem, M.A., Ul Haq, Z., Murtaza, B., Bakhat, H.F., 2020. Quantification and risk assessment of heavy metal build-up in soil-plant system after irrigation with untreated city wastewater in Vehari, Pakistan. Environmental geochemistry and health 42, 4281-4297.

Shayegan, H., Ali, G.A., Safarifard, V., 2020. Amide-functionalized metal–organic framework for high efficiency and fast removal of Pb (II) from aqueous solution. Journal of Inorganic and Organometallic Polymers and Materials 30, 3170-3178.

Shi, Z., Xu, C., Guan, H., Li, L., Fan, L., Wang, Y., Liu, L., Meng, Q., Zhang, R., 2018. Magnetic metal organic frameworks (MOFs) composite for removal of lead and malachite green in wastewater. Colloids and Surfaces A: Physicochemical and Engineering Aspects 539, 382-390.

Sholehhudin, M., Azizah, R., Sham, A.S.S.M., Amiruddin, Z., 2021. Analysis of Heavy Metals (Cadmium, Chromium, Lead, Manganese, and Zinc) in Well Water in East Java Province, Indonesia.

Subramaniyam, V., Thangadurai, T.D., Lee, Y.I., 2022. Zirconium based metal-organic framework for the adsorption of Cu (II) ions in real water samples. Cleaner Engineering and Technology 9, 100526.

Tanihara, A., Kikuchi, K., Konno, H., 2021. Insight into the mechanism of heavy metal removal from water by monodisperse ZIF-8 fine particles. Inorganic Chemistry Communications 131, 108782.

Tong, S., Li, H., Tudi, M., Yuan, X., Yang, L., 2021. Comparison of characteristics, water quality and health risk assessment of trace elements in surface water and groundwater in China. Ecotoxicology and Environmental Safety 219, 112283.

Varol, S., Şener, Ş., Şener, E., 2021. Assessment of groundwater quality and human health risk related to arsenic using index methods and GIS: A case of Şuhut Plain (Afyonkarahisar/Turkey). Environmental Research 202, 111623.

Wang, K., Tian, Z., Yin, N., 2018. Significantly Enhancing Cu(II) Adsorption onto Zr-MOFs through Novel Cross-Flow Disturbance of Ceramic Membrane. Industrial & Engineering Chemistry Research 57, 3773-3780.

Wang, Y., Lin, K., Liu, Y., Deng, X., 2022. Nanocomposites of functionalized Metal−Organic frameworks and magnetic graphene oxide for selective adsorption and efficient determination of Lead(II). Journal of Solid State Chemistry 313, 123300.

Xu, C., Yan, H., Zhang, S., 2021. Heavy metal enrichment and health risk assessment of karst cave fish in Libo, Guizhou, China. Alexandria Engineering Journal 60, 1885-1896.

Xu, R., Jian, M., Ji, Q., Hu, C., Tang, C., Liu, R., Zhang, X., Qu, J., 2020. 2D water-stable zinc-benzimidazole framework nanosheets for ultrafast and selective removal of heavy metals. Chemical Engineering Journal 382, 122658.

Yan, Y., Chu, Y., Khan, M.A., Xia, M., Shi, M., Zhu, S., Lei, W., Wang, F., 2022. Facile immobilization of ethylenediamine tetramethylene-phosphonic acid into UiO-66 for toxic divalent heavy metal ions removal: An experimental and theoretical exploration. Science of The Total Environment 806, 150652.

Yaqub, G., Khan, A., Zishan Ahmad, M., Irshad, U., 2021. Determination of Concentration of Heavy Metals in Fruits, Vegetables, Groundwater, and Soil Samples of the Cement Industry and Nearby Communities and Assessment of Associated Health Risks. Journal of Food Quality 2021.

Yazdi, M.N., Dadfarnia, S., Shabani, A.M.H., 2021. Synthesis of stable S-functionalized metal-organic framework using MoS42-and its application for selective and efficient removal of toxic heavy metal ions in wastewater treatment. Journal of Environmental Chemical Engineering 9, 104696.

Yin, N., Wang, K., Li, Z., 2018. Novel melamine modified metal-organic frameworks for remarkably high removal of heavy metal Pb (II). Desalination 430, 120-127.

You, D., Shi, H., Peng, M., Yang, L., Shao, P., Yin, K., Wang, H., Luo, S., Luo, X., 2022. Metal-center effect induced efficient charge transfer of metal-organic framework for strengthening Sb(V) capture performance. Nano Research.

Yuan, Q., Wang, Y., Yuan, F., Jia, S., Sun, H., Zhang, X., 2022a. Water-stable metal organic framework-199@polyaniline with high-performance removal of copper II. Environmental Science and Pollution Research 29, 44883-44892.

Yuan, Y., Yu, J., Chen, H., Bang, K.-T., Pan, D., Kim, Y., 2022b. Thiol-functionalized Zr metal-organic frameworks for efficient removal of Fe3+ from water. Cell Reports Physical Science 3, 100783.

Zahidi, N.M., Ansari, A., Sargand, G.Y., Achak, J., 2020. Analysis Of Heavy Metals In Surface And Groundwater At Lashkergah City, Helmand–Afghanistan.

Zainol, N.F.M., Zainuddin, A.H., Looi, L.J., Aris, A.Z., Isa, N.M., Sefie, A., Ku Yusof, K.M.K., 2021. Spatial Analysis of Groundwater Hydrochemistry through Integrated Multivariate Analysis: A Case Study in the Urbanized Langat Basin, Malaysia. International journal of environmental research and public health 18, 5733.

Zhang, Y., Kang, X., Guo, P., Tan, H., Zhang, S.-H., 2022. Studies on the removal of phosphate in water through adsorption using a novel Zn-MOF and its derived materials. Arabian Journal of Chemistry 15, 103955.

Zhang, Y., Wang, X., 2021. Evaluation of Heavy Metal Pollution in Shallow Groundwater of Farmland in Huaibei Plain, China. E3S Web of Conferences. EDP Sciences, p. 02009.